\documentstyle[epsf,11pt,fullpage]{report}

\begin{document}

\begin{center}

{\bf NELSON, NAGLE, CARROLL, IRWIN}

{\bf DIGIAL LOGIC CIRCUIT ANALYSIS AND DESIGN}

{\bf ERRATA}

Last Update - 04/11/02
\end{center}



{\bf Asterisk *} indicates errata reported after 4-1-96, when 
corrections were made for the first reprint. {\bf Double asterisk **}
indicates new errata reported in 2002.


\begin{description}


\item[Pg. 63.]   Table 1.11.  At the very top, move the subscript 4 
	to the left so that the column label reads $c_6c_5c_4$.

\item[Pg. 93.]   Table 2.4(b).  The label 11 on the 3rd row of the table
          should be changed to 10, and the label 10 on the bottom row
          of the table should be changed to 11.

\item[*Pg. 106.] Figure 2.4, Symbol Set 2.  Remove input b from the NOT
          gate. This gate should have only one input, a.

\item[*Pg. 170.] Problem 2.26. Change f(A,B,C) to f(A,B,C,D).

\item[*Pg. 180.] Example 3.4, 2nd line. There should be a "Sigma" symbol 
          in front of the minterm list: $\sum m(0,3,5,7,10,11,12,13,14,15)$.

\item[*Pg. 182.] 4th line from the bottom. There should be a "Sigma" symbol 
          in front of the minterm list: $f(A,B,C) = \sum m(2,6,7)$.

\item[*Pg. 206.] 3rd line from the bottom, end of the line. Change $y_3$ to $y_1$.

\item[*Pg. 241.] Problem 3.60, both parts (a) and (b). Change f(A,B,C,D) to
          f(A,B,C,D,E).

\item[**Pg. 252.] Line 11 - Change "73138" to "74138".
  
\item[Pg. 253.]  Figure 4.8 (d).  The inversion bubbles (circles) should be
          removed from inputs A, B, C, and G1 on the left side
          of the 74LS138 logic symbol. 

\item[Pg. 255.]  Figure 4.9 (d).  The inversion bubbles (circles) should be
          removed from inputs A, B, C, D on the upper left side
          of the 74154 logic symbol. 

\item[Pg. 267.]  Figure 4.21 (a) and (c). Enable input El should be
	  labelled EI.

\item[*Pg. 273.]  Remove inversion bubbles from the outputs of the
	  NAND gates connected to inputs E2-E15.  These should be AND
	  gates.

\item[*Pg. 275.]  Figure 4.27 (d).  Change "Strong" to "Strobe" at 1G-bar
	enable.

\item[*Pg. 275.]  Figure 4.27 (e).  Label "1G" and "2G" enables as active
	LOW.  The correct pin number for the 1Y output is 7; the 2Y output
	should be labeled pin 9.

\item[*Pg. 276.]  Figure 4.28 (a).  Label pin 4 output as "1Y" and pin 14
	input as "4A."

\item[*Pg. 280.] Figure 4.32 caption and Figure 4.32 (b).  Change lower case 
	x to capital X for consistency in the example.

\item[Pg. 327.]  Problem 4.41.  Change ``(Hint: Use the cascade inputs to
          compare the two least significant digits; use one AND gate.)"
          to read ``(Hint: Use the cascade inputs to compare the two most
          significant digits.)"

\item[**Pg. 398.] Figure 4.28(c). Remove the NOT gate at the bottom input
          to the R input of the bottom NOR gate.

\item[*Pg. 406.] Figure 6.22 (b).  The arc from state 1 back to state 1
	should be labelled ``d0" instaed of ``0d".

\item[*Pg. 408.]  Figure 6.25 (b).  Change ``JR" to ``JK." 

\item[Pg. 410.]  Figure 6.28(b).  The flip-flop inputs are mis-labelled
	on the left side of the symbol.
	  Change the upper input name from Q to D and the lower input
	  name from Q to C.  Delete the '76 near the upper output.

\item[*Pg. 411.] Figure 6.30 (a).  Labels ``tPHL and tPLH" at the bottom
        of the timing digram should be swapped.

\item[*Pg. 411.] Last sentence on the page reads ``...values for both
        $t_{PHL}$ and $t_{PLH}$, from the TTL manual [1], are listed 
        in Figure 6.30b
        as 0 ns."   Change to read ``...values for $t_{PHL}$ and 
        $t_{PLH}$, from the 
        TTL manual [1], are listed in Fig. 6.30b as 40 ns and 25 ns, 
        respectively."

\item[*Pg. 412.] First sentence reads ``...transferred to the flip-flop 
        output Q at the exact instant..."
	Change to read  ``...transferred to the flip-flop output Q at 
        either 40 ns or 25 ns from the exact instant..."

\item[*Pg. 420.] Middle of the page - Change capacitor value from
        C=$3.125 \mu F$ to $0.1067 \mu F$.

\item[**Pg. 437.] Figure 7.3(b) - under the table heading "Outputs",
        the time should read $t_{n+8}$ instead of $t_{n}+8$ (the 8 is
        part of the subscript).

\item[**Pg. 439.] End of line 11 - change "flip-flips" to "flip-flops".

\item[**Pg. 444.] Figure 7.6(d). The pulse on Data line F should not
        be there, since the value is "L" (low).

\item[**Pg. 457.] Line 15. The subscript for the second clear line should
        be 0(2) instead of O(2) (zero instead of letter O).

\item[*Pg. 466.] Figure 7.19 (c).  Fix three errors on the wire driven
	by $\overline{Clear}$ near the bottom left of the figure.

\begin{enumerate}
\item Change the inverter driven by $\overline{Clear}$ to a buffer by
	adding an inversion bubble to its input.

\item Remove the first dot to the right on the wire driven by this inverter.
      (The inverter output should not be connected to the vertical wire
       driven by the AND gate below it.)

\item Find the vertical wire connected to the upper three flip-flop
      CLR inputs.  This should also be connected to the wire driving
      the bottom flip-flop CLR input, and not to the wire immediately
      below it (i.e. move the vertical wire and dot 
      up from the feedback wire driven by the QD output.)
\end{enumerate}

\item[**Pg. 473.] Figure 7.23. Below the logic diagram, change (a) to (c).
      Also, the lower Q output of flip-flop C in that diagram should have 
      an inversion bubble (Q-bar output).

\item[Pg. 492.]  Figure 7.36(c).  In the logic diagram, at the left bottom,
          the AND gate whose inputs are Strobe (10) and Clock (9)
          should have inversion bubbles on both inputs.

\item[Pg. 498.] Problem 7.1.  The problem refers to Fig. 4.29.  This
	should be changed to Fig. 4.34.

\item[Pg. 500.] Problem 7.15 refers to Problems 7.8, 7.10, and 7.12.  These
         should be Problems 7.9, 7.11 and 7.13.

\item[Pg. 500.] Problem 7.16 refers to Problems 7.9, 7.11, and 7.13.  These
         should be Problems 7.10, 7.12 and 7.14.

\item[Pg. 500.] Problem 7.16 refers to Fig. 7.34b  and then to Fig. 7.34.
             These should be Fig. 7.34 and Fig. 7.34c, respectively.

\item[**Pg. 508.] Line 17 - Change "Fig. 8.1b" to "Fig. 8.1".

\item[*Pg. 532.] Figure 8.30, in the K-map for R2, change the entry in the
      top row (row 00), right column (column x=1), from ``0" to ``1".

\item[Pg. 623.] Problem 9.10, 2nd line, change ``using the given state assignment"
         to ``using each of the three unique state assignments", and then
         delete the state assignment given next to the state table.

\item[Pg. 677.] Problem 10.10, 3rd line presently reads ``If $x_2 = 1$ and $x_2$
         changes from 0 to 1..."  The first subscript should be changed to
         1 so as to read: ``If $x_1 = 1$ and $x_2$ changes from 0 to 1..."

\item[Pg. 680.] Problem 10.17.  The bottom row of the excitation table should
         be labelled 11 and the next row up should be labelled 10,
         to correspond with the circled stable states in those rows.

\item[Pg. 735.] Figure P11.8.  The AND gate driving flip-flop clock input C1
         should be changed to a NAND gate (add an inversion bubble to
         its output.)

\item[Pg. 737.] Problem 11.25 change ``PDL state machine model" to ``PDL model".

\item[Pg. 742.] Last paragraph reads ``A test $T_i$ for fault $p/d$ is...''.
	Change the subscript on the $T$ from $i$ to $j$, , i.e. change $T_i$
        to $T_j$.

\item[Pg. 776.] Figure 12.26.  At the top left, the 2-to-1 multiplexer selecting
         between Scan-in and the feedback signal should have a control
         input connected to input line B1.

\item[Pg. 785.] Figure P12.15.  The OR gate input marked $\beta$  should be
         connected at its left end to the vertical line corresponding
         to y2, rather than to line y1. 

         Also, at the output of the inverter driven by flip-flop output y3
         there should be a ``dot" to show a connection to the vertical
         line that ends there. (The other end of the line connects to
         the gate input marked $\alpha$.)

\end{description}
\end{document}    



